ASC 6.5 Meter C band Antenna.

1 EA 4LPNC-65 4PORT COMBINER & FEED SYSTEM

1 EA ES65-2 6.5M ANTENNA ASSEMBLY

1 EA 201630 Anchor Bolt Kit for 5.6/7.3/7.6 Meter Earth Station Antennas with Tripod Mount and ES45T-HW-1, 4.5M High Wind Antenna

1 EA LRK9 Lightning Rod Kit For4.9/5.6/6.5/7.3/7.6/8.1/9.3/9.4M ESA. Includes Air and Universal Terminals, connectors, clamps and necessary Hardware

1 EA ANTGND-9 Foundation Installed Grounding Kit For 5.6/7.3/7.6/8.1/9.3/9.4M ESA.

1 EA PK9DRA Dual Reflector Polarization Drive Kit for 7.3/7.6/8.1/9.3/9.4M Antennas. Nom. Speed (Deg/Sec): 2.2 at 60Hz; 1.8 at 50Hz 100-115 VAC, 50-60 Hz Nominal 40 Watts, Single Phase

2 EA 208349 RESOLVER

1 EA XAPC-76 SINGLE RUN POLARIZATION AND CROSS AXIS WAVEGUIDE, 7.6M C-BAND. USE WITH 2-PORT C-BAND

FEEDS.

1 EA XAPC-76-UPG UPGRADE TO XAPC-76. PROVIDES SECOND RUN OF WAVEGUIDE TO ACCOMMODATE 4-PORT

7.6 M C-BAND FEEDS. PURCHASE IN ADDITION TO XAPC-76.

1 EA MK7VS-208 Variable Speed Motorization. 200-230 VAC, 3 Phase, 50/60 Hz.4 Conductor (3 ph Delta + safety Ground) or

5 Conductor (3 ph WYE + safety ground). Use with 5.6/7.3/7.6M Earth Station Antennas. Use with ACS400-xxx Controllers. Fast 0.5 Degrees/Second, Az/El Slow, 0.05 Degrees/Second, Az/El Safety Ground Required

1 EA 206505 Anchor Bolt Template for 5.6/7.3/7.6 Meter Earth Station Antennas with Tripod Mounts and ES45T-HW-1, 4.5M High Wind Antenna.